**JACKON THERMOMUR Post-Pour Checklist**

|  |  |  |
| --- | --- | --- |
| 1 | Are the walls straight and true? |  |
| 2 | Are all the openings plumb, have they been checked? |  |
| 3 | Is the consolidation complete? |  |
| 4 | Has the top been levelled? |  |
| 5 | Have all the anchors, wall plates. Joist hangers etc, been fitted? |  |
| 6 | If the wall is to be continued, are the rebar laps protruding to the right length? |  |
| 7 | Has all the kit been thoroughly cleaned including the bracing? |  |
| 8 | In cold weather, has the top of the wall been protected from frost penetration? |  |